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	Phase
	A (Activities)
	SU
	Name/brief description
	Prior to
	Contemporary to
	Later than

	Phase Ia
12th–13th centuries
	A100
Main chapel and beginning of the north-western façade
	001
	[bookmark: _heading=h.e1dodhnsclvd]Wall of the main chapel, built in granite ashlar masonry arranged in horizontal courses, finished with a cavetto cornice supported by six cavetto corbels. They are decorated with spheres and geometric motifs on its north-western and south-eastern façades. The north-eastern elevation, contains a slit window.
	002, 003, 004, 005, 006, 008, 009, 012, 045, 046, 047?, 048, 049, 050, 051, 052,  053, 054, 055, 056, 057, 058, 059, 060, 061, 079, 104, 105, 108, 109,
	043
	

	
	
	007
	Antefixed stone cross on the north-eastern wall of the main chapel.
	006
	
	001

	
	
	043
	Remains from the beginning of the north-western façade of the nave, built in granite ashlar masonry that continues the courses of the apse.
	006, 010, 042, 060, 061, 099, 117
	001
	

	
	
	113
	Original wall of the presbytery, above the current pointed arch, built in granite ashlar masonry laid in horizontal courses.
	012, 050, 063, 096, 098, 099
	001, 043
	

	
	A101
Floor of the Main Chapel
	104
	Stone flooring in the chancel. Elements with different shapes and sizes.
	062, 103, 105
	
	

	
	
	105
	Raised stone platform on the chancel floor.
	107
	
	104

	
	A102
Altar base
	107
	Altar stand/ reused Roman ara.
	
	
	105

	Fase Ib
13th-14th centuries
	A103
Nave of the church
	012
	Wall of the nave built in granite ashlar masonry arranged in undulating courses, finished on the north-western and south-eastern façades with a rectangular-profile cornice and cavetto corbels, undecorated and larger than those used in the apse. It contains three lintelled doorways on the north-western, south-eastern, and south-western façades and, above the south-western and north-western doors, a narrow slit window. The plan of the nave does not share the same orientation as the apse; it is rotated toward south.
	006, 010, 011, 015, 016, 019, 020, 021, 022, 024, 025, 026, 027, 028, 029, 030, 031, 034, 035, 036, 037, 038, 039, 040, 041, 060, 061, 063, 064, 065, 066, 067, 068, 069, 070, 071, 072, 074, 075, 076, 077, 078, 079, 085, 086, 087, 088, 089, 090, 091, 092, 093, 094, 095, 102, 119, 120, 121
	
	001, 013, 042, 112, 113

	
	
	013
	Foundation supporting the south-eastern façade of the nave (left side of the door).
	003, 012, 014
	112
	

	
	
	042
	Break interface of the primitive nave (SU043), contemporary with the apse SU001.
	012, 010
	
	043

	
	
	112
	Foundation supporting the south-eastern façade of the nave (right side of the door).
	003, 012, 014, 061
	013
	

	
	A104
Renovation of the chancel arch
	060
	Pointed arch with voussoirs and the impost from which it rises, built in granite ashlar masonry. 
	
	
	001, 012, 043, 061, 099

	
	
	061
	Ashlar masonry pillars on which the presbytery arch rests.
	060
	
	001, 012, 043, 099, 102

	
	
	098
	Closing the interior window over the presbytery arch.
	113
	
	

	
	
	099
	Interface - tear in the wall to place the SU060 arch on the south-western elevation of the nave.
	060
	
	113

	
	
	102
	Interface - cut -out in the nave floor, near the chancel, NE angle.
	061
	
	101

	
	A105
Floor of the nave
	101
	Stone floor in the nave, different shape and dimensions, some elements reused.
	061, 062, 102, 103, 106, 119 
	
	012, 043, 112

	
	A106
Porch attached to the south-eastern façade of the nave
	015
	Console n.º 2, from west to east, on the nave south-eastern façade.
	017
	
	012

	
	
	016
	Console n.º 1, from west to east, on the nave south-eastern façade.
	018
	
	012

	
	
	017
	Interface - cut-out in console n.º 2 to fit the side porch support beam.
	
	
	015

	
	
	018
	Interface - cut-out in console n.º 1 to fit the side porch support beam.
	
	
	016

	
	
	019
	Interface - In-line holes under the cornice on the nave south-eastern façade.
	
	
	012

	
	A107
The Stations of the Cross carved 
	079
	Crosses engraved (via sacra) on the ashlars inside the church (nave and main chapel).
	
	
	001, 012

	
	A108
Undetermined hole
	021
	Interface - hole in the south-eastern wall of the nave, in the fifth row, next to the chancel.
	022
	
	012

	
	A109
Remains of the fixing of the first south-eastern and south-western doors of the nave
	075
	Interface - hole torn to insert hinges (SU076) from a previous door on the south-eastern elevation of the nave. Right side, lower part of the jamb.
	
	
	012

	
	
	076
	Hinges of a former door on the south-eastern elevation of the nave. Right side, upper part of the jamb.
	
	
	012

	
	
	083
	Interface - hole in the nave's south-western elevation, to the right of the access opening, in the fourth course of the jamb, possibly from an earlier door.
	
	
	012

	
	
	091
	Interface - circular hole in the nave's south-western elevation, related to the iron metal element that reinforced the door's closure. Right side, possibly from an earlier door.
	
	
	012

	Phase II
15th–16th centuries
	A200
Single-arch bell gable
	030
	Interface - cut-out in the cornice that lines the wall of the nave façade.
	031
	
	012

	
	
	031
	Supporting embankment related to the possible access staircase to the bell-gable.
	033
	
	012, 030

	
	
	032
	Single-arch bell gable with a triangular gable top, built in granite ashlar masonry. The arch rises from a chamfered impost.
	
	
	010, 012, 031

	
	
	033
	Bell and its wooden support.
	
	
	032

	
	A201
Access to the belfry via the south-western façade
	029
	Interface - holes in the façade of the nave related to some structure that covered the entrance.
	034
	
	012

	
	A202
Mark left by the bell rope rubbing against it
	027
	Interface - Abrasion mark on the nave façade produced by the rope used to ring the bell
	028
	
	012

	
	A203
Renovation of the south-eastern door of the nave
	071
	Interface - circular hole cut into the south-eastern and south-western wall of the nave, to the right of the access opening, in the 4th row.
	
	
	012

	
	
	072
	Interface (cut) in the south-eastern and south-western wall of the nave, to the left of the access opening, in the second and third courses.
	073
	
	012

	
	
	073
	Filling the SU072 interface.
	
	
	072

	
	
	074
	Interface - cut in the south-eastern and south-western wall of the nave, to the right of the access opening, in the first courses.
	024
	
	012

	
	
	077
	Interface - cut-out on the south-eastern elevation of the nave. Right side, middle part of the jamb.
	024
	
	012

	
	
	081
	Interface - cut-out on the south-eastern elevation, west of the door.
	
	
	012

	
	A204
Renovation of the west door of the nave
	084
	Interface no. 1 – cut in the south-western elevation, on the right side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	
	085
	Interface no. 2 – cut in the south-western elevation, on the right side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	
	086
	Interface no. 3 – cut in the south-western elevation, on the right side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	
	087
	Interface no. 1 – cut in the south-western elevation, on the left side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	
	088
	Interface no. 2 – cut in the south-western elevation, on the left side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	
	089
	Interface no. 3 – cut in the south-western elevation, on the left side of the door, from top to bottom, for the fixing of the wooden door.
	
	
	012

	
	A205
Renovation of the north-western door of the nave
	092
	Interface - repair opening/door in north-western elevation. Possible removal of a wooden lintel?
	093
	
	012

	
	A206
Construction of a high choir at the western end of the nave
	078
	Interface - holes cut into the north-western elevation to support a high choir.
	
	
	012

	
	
	120
	Negative related to the existence of a choir on the south-western elevation of the nave (internal side of the façade).
	
	121
	012

	
	
	121
	Negative related to the existence of a choir on the north-western elevation of the nave (internal side of the façade).
	
	120
	012

	
	A207
Renovation of the chancel roof
	114
	Refurbishment of the east elevation of the chancel (internal side of the façade), built in granite ashlar masonry.
	
	
	001

	
	A208
Almsbox
	100
	Wooden alms box placed on the west elevation of the presbytery.
	
	
	061

	Phase IIIa
Before 1952
	A300
Installation of a lighting system in the Main Chapel
	049
	Interface - circular holes torn in the exterior south-eastern wall of the main chapel (cable fixing).
	
	
	001

	
	
	053
	Interface - perforation in the side walls of the main chapel (electricity cables).
	
	
	001

	
	
	054
	Electrical outlet on the south-eastern elevation of the chancel.
	
	
	001

	
	
	055
	Light switch, south-eastern elevation of the nave.
	
	
	001

	
	
	066
	Light switch n.º 1 (W to E) in the south-eastern elevation of the nave.
	
	
	012

	
	
	067
	Light switch n.º 2 (W to E) in the south-eastern elevation of the nave.
	
	
	012

	
	
	108
	Lighting system of the chancel (2 lamps + chandelier), in the south-eastern elevation of the nave.
	050
	
	001

	
	
	116
	Light switch on the inner wall of the chancel, under the arch impost, on the west elevation of the presbytery.
	
	
	061

	
	
	117
	Cut for fitting the SU118 power socket, on the west elevation of the presbytery.
	118
	
	061

	
	
	118
	Electricity socket to the north-western of the west elevation of the presbytery.
	
	
	117

	
	A301
Installation of a lighting system in the nave
	080
	Electrical outlet on the south-eastern elevation of the nave, west of the door.
	
	
	012

	
	
	095
	Nave´s lighting system (bracket and 2 lamps) on the north-western and south-eastern elevation of the nave.
	
	
	012

	
	
	119
	Tear in the paving stones of the nave, in the SW corner.
	103
	
	101

	
	A302
Limewash finish on the walls
	009
	Traces of a white coating, possibly limewash or paint, identified on the cornice of the south-eastern elevation of the apse.
	
	
	001

	
	
	059
	Traces of a whitish wall coating preserved at the upper section of the south-eastern elevation of the chancel/apse.
	
	
	001, 124

	
	A303
Cross and its wooden base
	056
	Wooden stand and cross on the south-eastern elevation of the chancel.
	
	
	001

	Phase IIIb
First half of the 20th century
	A304
Cracks caused by neglect
	004
	Damage/crack in the chancel's 3rd corbel (west to east).
	
	
	001

	
	
	005
	Damage/crack in metope no. 1 (west to east) between chancels.
	
	
	001

	
	
	028
	Damage/vertical crack in the lintel of the nave south-western façade door.
	
	
	012, 027

	
	
	044
	Sub-horizontal damage/crack in the door lintel of the nave's south-eastern wall.
	
	
	012

	
	
	046
	Damage/vertical crack in one of the ashlars of the north-western wall of the main chapel/apse (3rd row).
	
	
	001

	
	
	111
	Lesion/crack in an ashlar block on the south-eastern wall of the nave (fourth course, north-eastern side).
	
	
	012

	Phase IIIc
Second half of the 20th century
	A305
Unspecified breaks and cuts and their repairs
Second half of the 20th century
	022
	Stone that fills the hole SU021.
	
	
	021

	
	
	034
	Stone filling one of the holes identified with SU029 on the façade of the nave
	
	
	029

	
	
	038
	Interface - hole in the north-western wall of the nave, east of the door
	039
	
	012

	
	
	039
	Filling of SU038 with a stone and mortar.
	
	
	012, 038

	
	
	040
	Interface - break over the door lintel of the north-western wall of the nave.
	041
	
	012

	
	
	041
	Break interface located above the lintel of the door in the north-western wall of the nave.
	
	
	012, 040

	
	
	051
	Interface - hole in an ashlar of the south-eastern elevation (inside the main chapel).
	052
	
	001

	
	
	052
	Stone that closes the hole SU051.
	
	
	001, 051

	
	
	057
	Interface - cut-out in the south-eastern elevation of the chancel, under the cross.
	058
	
	001

	
	
	058
	Filling of the cut-out SU057.
	
	
	001, 057

	
	
	090
	Filling the SU089 interface.
	
	
	012, 089

	
	
	098
	Closing the interior window over the presbytery arch.
	
	
	113

	
	A306
Opening windows in the nave and the installation of glass
	047
	Stone infill in the lower section of the arrow slit on the façade of the chancel (north-eastern wall).
	048
	
	001

	
	
	048
	Glass closing the arrow slit on the façade of the chancel (north-eastern wall).
	
	
	001, 047

	
	
	065
	Interface for opening a window in the south-eastern elevation of the nave.
	070
	
	012

	
	
	070
	Glass that closes the window UE065.
	
	
	065

	
	
	082
	Glass that closes the arrow slit in the south-western façade of the nave.
	
	
	012

	
	
	094
	Glass that closes the arrow slit in the north-western façade of the nave.
	
	
	012

	
	
	115
	Refurbishment of the original main chapel window (= SU047).
	048
	047
	001

	
	A307
Repair of the nave doors and installation of wooden locks
	024
	Rectangular wooden door in the opening of the south-eastern wall of the nave.
	
	
	012, 014, 074, 077

	
	
	026
	Rectangular wooden door in the opening of the west wall on the nave.
	
	
	012, 084, 085, 086, 087, 088, 089

	
	
	036
	Rectangular wooden door in the opening of the north-western wall of the nave.
	
	
	092

	
	
	064
	Interface in the area of the door and lintel on the north-western elevation of the nave.
	
	
	012

	
	
	093
	Interface - repair opening/door in north-western elevation of nave.
	036, 093
	
	012

	
	A308
Repair of the church floor and the thresholds of the doorways
	002
	Cement coating between the lower edge of the outer wall and the pavement (half cane).
	
	
	001

	
	
	003
	Stone pavement around the church.
	
	
	001, 012, 014, 025, 035, 042, 043

	
	
	014
	Sill of the nave´s south-eastern wall opening.
	003, 024
	
	012

	
	
	025
	Sill of the nave´s south-western wall opening.
	003, 026
	
	012

	
	
	035
	Sill of the nave´s north-western wall opening.
	003, 036
	
	012

	
	
	106
	Cement that fills the joints in the main nave floor.
	103
	
	101

	
	
	062
	Sill between the main chapel and the nave, under the SU060 presbytery arch.
	103
	
	061, 101, 104

	
	A309
Upgrade to the lighting system
	103
	Electricity cable in the ground of the church.
	
	
	012, 014, 025, 062, 101, 104, 106

	
	A310
Wooden roof

	010
	Oldest roof of the church nave.
	011
	
	012, 031, 042, 043

	
	
	050
	Main chapel roof timbering.
	006
	
	001, 060, 113, 114

	
	
	063
	Nave roof timbering.
	010, 011
	
	012, 096, 097, 113

	
	
	096
	Interface - cut-out for repairing the roof, over the presbytery arch.
	063, 097
	
	113

	
	
	097
	Filling of SU096 with a stone and mortar wall.
	
	
	096, 113

	
	
	098
	Closing the interior window over the presbytery arch.
	
	
	113

	
	A311
Repairing joints with cement
	020
	Cement level that fills the joints in the external walls of the building.
	
	
	012

	Phase IIId
Late 20th and early 21st centuries
	A312
Roof renovation
	006
	Roof (tiles) of the main chapel/apse.
	
	
	001, 007, 009, 012, 050 

	
	
	008
	Cement level that waterproofs the roof in contact with the eaves.
	
	
	001, 006, 012, 043, 045

	
	
	011
	Renovation of the nave roof in the area closest to the eaves.
	
	
	010, 012, 030, 031

	
	
	045
	Metal sheet for waterproofing the chancel between the roof and cornice.
	
	
	001, 006, 008, 043

	Not linked to a phase
	Not linked to an A
	021
	Interface - hole in the south-eastern wall of the nave, in the fifth row, next to the apse.
	022
	
	012

	
	
	023
	Interface - hole under the lintel of the opening in the south-eastern wall of the nave.
	
	
	012

	
	
	037
	Interface - hole in the north-western wall of the nave, west of the door.
	
	
	012

	
	
	038
	Interface - hole in the north-western wall of the nave, east of the door.
	039
	
	012

	
	
	040
	Interface - break in the door lintel of the north-western wall of the nave.
	041
	
	012

	
	
	051
	Interface - hole in an ashlar of the south-eastern elevation (inside the main chapel).
	052
	
	001

	
	
	068
	Recess in one of the ashlars on the north-western elevation of the nave, to the east of the access door.
	
	
	012

	
	
	069
	Recess in one of the ashlars on the north-western elevation of the nave, to the west of the access door.
	078?
	
	012

	
	
	109
	Interface - holes in the north-western elevation of the main chapel / apse.
	
	
	001

	
	
	110
	Interface - tear in the south-eastern elevation of the main chapel / apse.
	
	
	001



